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INSTRUCTIONS FOR SETTING UP THE INOX CLOSING DEVICE

serie JUGO
Inox manual closing device MOD. JUGO is intended for closing up larger diameters of corks (30 – 37mm). An innovation of the inox JUGO closing device is in the vertical closing of the closing head, which provides an easier and greater quality closing up of the cork.
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Inox manual closing device MOD. JUGO can close up the following types of bottles: 

1) BORDOLESE  ITA. 3L,  5L

2) BORGUNDER        3L,  5L, 

3) BORD. FRANCESE  9L, 12L, 18L

When closing up the above-listed bottles the additional settings on the closing device shall be taken into account. 
The closing device consists of the following components: 

· 1 piece ADJUSTABLE TABLE LARGE -  intended for the bottles BORD FRANCESE  9L, 12L, 18L 

· 1 piece ADJUSTABLE TABLE SMALL – intended for the bottles BORD ITA. 3L, 5L

· 1 piece ADDITIONAL FITTING SHORTER for the adjustable table – intended for the bottles BORD. FRANCESE 9L, 12L

· 1 piece ADDITIONAL FITTING LONGER for the adjustable table – intended for the bottles BORD. ITA. 3L, 5L

· 1 piece TEFLON LINED INSERT PIECE SMALL of diameter 21mm (for closing the bottles BORD. ITA. 3L, 5L)

· 1 piece TEFLON LINED INSERT PIECE LARGE of diameter 28mm (for closing the bottles BORD. FRANCESE 9L)

1) INSTRUCTIONS FOR CLOSING UP THE BOTTLES:

· BORD. FRANCESE 18L (the basic fitting for the table + large table without the teflon lined insert piece under the closing retaining device) 

· BORD. FRANCESE 12L, (the basic fitting for the table + additional fitting shorter + large table without the teflon lined insert piece under the closing restraining device)

· BORD. FRANCESE 9L (the basic fitting for the table + additional fitting shorter + large table with teflon lined insert piece under the closing restraining device of 28 mm diameter)

· BORD. ITA 3L, 5L, (the basic fitting for the table + small table with additional longer fitting + teflon lined insert piece under the closing restraining device of 21 mm diameter)

2) SETTING UP THE DEPTH OF THE IMPRESSION (see figure 1)

Setting up the depth of the impression of the cork is determined by setting up the nut.
3) SETTING UP THE INCLINATION OF THE NECK OF THE BOTTLE (see figure 2)

The bottle is placed on the table and is then fixed under the closing restraining device. A relevant teflon lined insert piece (bearing in mind the type of the bottle) is affixed under the restraining device. In the event of bottles BORD. FRANCESE  12L, 18L, the teflon lined insert piece is not required. The external diameter of the neck of the bottle shall be no more than 50mm.

4) SETTING UP THE HEIGHT OF THE BOTTLE BEARING DEVICE (see figure 3)

The congestion of bottles of different height enables setting up the height of the bottle bearing device by moving the handle. In doing so special attention shall be paid so that the bottle is always firmly affixed under the closing restraining device.

5) SETTING UP THE CLUTCH  (see figure 4)

Closing devices are equipped with an adjustable clutch. As time passes by the lever of the clutch gets tired causing the bottle to settle well during closing. The distance between the nuts shall always be 15mm. With setting up the nuts we lower the lever into a lower position, which enables us to reach correct operation.

TYPES OF BOTTLES: BORD. ITA 3L, 5L,  BORD. FRANCESE 9L, 12LČ, 18L
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COMPONENTS: 



Shorter adjustable                  
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Cork:


Diameter:           D   30-37 mm


Height max.        H        55 mm 








Bottles:


Diameter A:         min. A        22 mm     


Diameter B:         max.B        43 mm 


Diameter D:         max.D      200 mm


Height:            max. H 400   790 mm








TEFLON LINED INSERT PIECE


presentation of setting up the teflon lined insert piece (large 28mm, small 21mm) under the closing restraining device








ADJUSTABLE TABLE 


(large, small with a longer adjustable lengthening piece)





Shorter adjustable 


lengthening piece
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